#
NO.18 JUDDER UPON TORQUE CONVERTER CLUTCH (TCC) OPERATION

BHE050301026W23

18 | Judder upon torque converter clutch (TCC) operation
DESCRIPTION | • Vehicle jolts when TCC is engaged.
POSSIBLE CAUSE | Caution • If the TCC is stuck, inspect it. In addition, inspect the oil cooler for foreign particles which may have mixed in with the ATF. • TCC piston slips due to burning. • The malfunction is basically the same as for No.14 "TORQUE CONVERTER CLUTCH (TCC) NON-OPERATION".