#
ON-BOARD DIAGNOSTIC SYSTEM (IMMOBILIZER SYSTEM) PID/DATA MONITOR FUNCTION

BHE091401077T06

• The following items can be verified:

  – Number of continuous DTCs
  – Number of key ID numbers registered with the vehicle

• Use the WDS to read the PID/data monitor.

## PID/Data Monitor Table

PID name (definition) | Detected condition
--- | ---
CCNT_DD (Number of continuous DTCs) | • DTCs are detected: 1-255 • No DTCs are detected: 0
NUMKEYS (Number of key ID numbers registered with the vehicle) | Number of key ID numbers registered: 0-8