#
LIGHTS-ON REMINDER WARNING ALARM CONSTRUCTION/OPERATION

BHE092255430T08

## System Wiring Diagram

1 | Instrument cluster
2 | TNS relay
3 | Light switch
4 | Buzzer
5 | Microcomputer
6 | Door switch (driver's side)
7 | AND

## Operation

• The buzzer in the instrument cluster sounds continuously when all the following three conditions are met:

  – The ignition switch is in the LOCK or ACC position.
  – The headlight switch is in the TNS or headlight position.
  – The driver-side door is open (driver-side door switch is on).

  Note

  • When the conditions for the lights-on reminder warning and the key reminder warning alarms are present at the same time, the key reminder warning alarm is given first priority.