#
POWER WINDOW SYSTEM INITIAL SETTING

BHE091266350W01

  Note

  • A driver-side window will not fully close automatically under following the conditions:

  – The battery has been disconnected during vehicle maintenance or for other reasons.
  – The power window main switch connector have been disconnected.

  • Carry out the following procedure to resume operation:

1. Turn the ignition switch to the ON position.

2. Press the driver-side power window main switch and fully open the driver-side window.

3. Pull up the driver-side power window main switch to the manual-up position to fully close the driver-side window, and keep holding the switch up at the position for approx. 2 s to complete initial setting.