#
TROUBLESHOOTING INDEX

BHE070301038W02

No. | TROUBLESHOOTING ITEM | DESCRIPTION
--- | --- | ---
1 | Insufficient air (or no air) blown from vents. | • Problem with each vent or duct or both. • Airflow mode does not change.
2 | Amount of air blown from vents does not change. (Full-auto air conditioner) | • Malfunction in blower system.
3 | Amount of air blown from vents does not change. (Manual air conditioner) | • Malfunction in blower system.
4 | Air intake mode does not change. | • Air intake mode does not change when switching REC/FRESH mode.
5 | No temperature control with A/C amplifier. | • Temperature does not change when operating temperature control dial.
6 | Windshield fogged. | • A/C compressor does not operate while airflow mode is in DEFROSTER or HEAT/DEF modes. • Air intake mode does not change to FRESH while airflow mode is in DEFROSTER or HEAT/DEF modes.
7 | Air from vents not cold enough. | • Magnetic clutch operates but A/C system malfunctions.
8 | No cool air. | • Magnetic clutch does not operate.
9 | Noise while operating A/C system. | • Noise from magnetic clutch, A/C compressor, hose or refrigerant line.