#
BASIC SYSTEM OUTLINE

BHE071101040T01

Reduced Weight

• A/C unit with integrated cooling and heater units adopted to reduce weight.

Improved Air Conditioning Performance

• Sub-cooling system with an integrated condenser and receiver/drier adopted to facilitate evaporator operation. This system also reduces the number of parts and the amount of refrigerant.

Improved Comfort

• Air filter, which cleans air flowing into passenger compartment, adopted.