#
REAR BUMPER REINFORCEMENT REMOVAL/INSTALLATION

BHE091050070W02

1. Remove the following parts:

  (1) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)
  (2) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)
  (3) Rear combination lights (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)
  (4) Rear bumper (See REAR BUMPER REMOVAL/INSTALLATION.)

2. Remove the nuts, then remove the rear bumper reinforcement.

3. Install in the reverse order of removal.