AF481-7546 ex2 is.. STI7 JDM

1.4 bar boost done in the summer (27 deg ambient).
It has Full decat exhaust with a 0.9mm restrictor (standard size on STI) in the boost pipe from the compressor housing to the boost solenoid "T" Piece.
It was also fitted with a "High Flow" fuel pump which is MUST on any STI with Full Decat Exhaust system.
Power output is around 330bhp and 300 lbs.ft torque (400NM).
