BODY STRUCTURE
BS

BODY STRUCTURE > General Description
SPECIFICATION

Refer to “Body Repair Manual” for general description of body structure, reference points and reference dimensions.

BODY STRUCTURE > Plug / Grommet Sheet
COMPONENT
1. UPPER FACE 1

(1) | Plug | (4) | Plug | (7) | Grommet sheet
(2) | Grommet sheet | (5) | Grommet sheet | (8) | Plug
(3) | Plug | (6) | Plug |  |

2. UPPER FACE 2

(1) | Plug (without rear seat heater) | (4) | Plug | (7) | Grommet sheet (without rear seat buckle switch)
(2) | Grommet | (5) | Grommet sheet (without keyless access system or without rear seat buckle switch) |  |
(3) | Grommet sheet (without keyless access system or without rear seat buckle switch) | (6) | Grommet sheet (without rear seat buckle switch) |  |

3. LOWER SURFACE

(1) | Plug | (4 | Plug | (7) | Plug
(2) | Plug | (5) | Plug | (8) | Grommet sheet
(3) | Plug | (6) | Plug | (9) | Plug

4. SIDE SURFACE

Illustration indicates the RH side. The structure of LH side is symmetrical.

(1) | Grommet sheet | (4) | Plug | (7) | Plug
(2) | Plug | (5) | Plug | (8) | Plug
(3) | Plug | (6) | Plug |  |

5. OBLIQUE VIEW 1

Illustration indicates the RH side. The structure of LH side is symmetrical.

(1) | Plug | (2) | Grommet sheet |  |

6. OBLIQUE VIEW 2

The structures of (3) and (4) are symmetrical.

(1) | Grommet sheet | (3) | Plug (without Blind Spot Detection/Rear Cross Traffic Alert system, without keyless access system, without rear fog light, without Reverse Automatic Braking) | (4) | Plug (without sunroof)
(2) | Plug (without sunroof) |  |  |  |

7. FRONT SIDE / BACK SIDE

(1) | Plug | (2) | Plug | (3) | Plug

8. INDOOR

The structures of (1), (2) and (3) are symmetrical.

(1) | Plug | (3) | Grommet sheet | (5) | Plug
(2) | Plug | (4) | Plug | (6) | Plug